// Sample options.txt configuration file for Pi1541



// If you would like to change the drive number then specify it here (8 is the default)
//deviceID = 9

// If you are using the split line hardware option (ie Option B) then you need to specify this option
splitIECLines = 0
// If you are using some type of hardware that requires the lines to be inverted then specify these options here
//invertIECInputs = 1
//If you are using a 7407
//invertIECOutputs = 0

// If you are using the Pi's composite video out then these options allow you to experiment with the display resolution
//ScreenWidth = 512
//ScreenHeight = 384

// By default Pi1541 will search the root of the SD card for a ROM file and use this for ROM1.
// The first file found with either of the following names will be used; d1541.rom, dos1541, d1541II, Jiffy.bin
// You can override the default ROM1 by specifying it here
//ROM1 = YourDefaultRom
// You can specify additional ROMS here (up to 7)
// You can then use the function keys (F1-F7) on the keyboard to change which one you would like to use (only in browse mode and not in emulation mode)
// You can also use the buttons to swap ROMs by holding down button 1 and pressing one other buttons 2-5
// .LST files can also specify one of these ROMS that will automatically selected when the LST file is loaded.
//ROM2 = Jiffy.bin
//ROM3 = d1541II
ROM1581 = 1581-rom.318045-02.bin

// The rate (in seconds) a long selection is scrolled
scrollHighlightRate = 0.07

// Enable RAMBoard emulation - 8k drive RAM expansion at 0x8000
//RAMBOard = 1

ChargenFont = chargen		// 8 bit font file

// If using CBMFileBrowser then it is best to specify this option. When the computer resets the Pi will always revert back to the root folder ready to load CBMFileBrowser again.
OnResetChangeToStartingFolder = 1

// If you use FB64 (CBMFileBrowser) and want to use a fast loader cartridge (AR6, EFL, FC3) to load it then use this option to automatically mount it. 
// You MUST have a disk image in \1541 with this filename
autoMountImage = fb.d64 
// If you are using a FB128 in 128 mode you can get FB128 to auto boot using this option
// AutoBootFB128 = 1

// If you are using a 128 you can auto boot anything using this option
// This over-rides AutoBootFB128
// 128BootSectorName = bootsect.128

// If you would ever like to disable browse mode completely ypu can do so here
// DisableSD2IECCommands = 1

// This option displays the IEC bus activity on the bottom of the Pi's screen
GraphIEC = 1

// If you have hardware with a peizo buzzer (the type without a generator) then you can use this option to hear the head step
SoundOnGPIO = 1
SoundOnGPIODuration = 100 // Length of buzz in micro seconds
SoundOnGPIOFreq = 200 // Frequency of buzz in Hz

// You can create 320x240 PNG files with the same name as your disk images. With this option turned on they will be displayed on the Pi's screen.
//DisplayPNGIcons = 1

// If you would like to specify what file will be loaded by LOAD"*" in browse mode then specify it here
StarFileName = fb.d64

// Alt-N creates a new diskimage.
// Names are formed automatically as autoname001.d64, autoname002.d64 etc...
// change the base of the filename here
//AutoBaseName = autoname

// If you are using a LCD screen then specify it here
LCDName = ssd1306_128x64
//LCDName = ssd1306_128x32
//LCDName = sh1106_128x64

// If you are using a LCD screen and you would like PageUp and PageDown keys to work with it (rather than the HDMI screen) then specify this option
//KeyboardBrowseLCDScreen = 1

// change startup logo on oled - 1541ii or 1541classic
//LcdLogoName = 1541ii
//LcdLogoName = 1541classic
//LcdLogoName = customfile.raw

// If you are using I2C LCD you can optionally change what pins it is connected to.
// (defaults to 0 for non-split lines (Option A) or 1 for split lines (Option B))
//i2cBusMaster = 0 //SDA - pin 27 SCL - pin 28
//i2cBusMaster = 1 //SDA - pin 3 SCL - pin 5
//i2cLcdAddress = 60	// I2C display address in decimal and shifted. 60 == 0x78, 61 == 0x7A
//i2cLcdFlip = 1 // Rotate i2c LCD screen 180 degrees
//i2cLcdOnContrast = 127 // Allows you to adjust the contrast on your i2c LCD screen
//i2cScan = 1 // scan i2c bus and display addresses on screen

//QuickBoot = 0		// faster startup
//ShowOptions = 0	// display some options on startup screen 
//IgnoreReset = 0

// You can remap the physical button functions
// numbers correspond to the standard board layout
//buttonEnter = 1
//buttonUp = 2
//buttonDown = 3
//buttonBack = 4
//buttonInsert = 5

//Gives you the option to use the font specified by the "ChargenFont" option on the OLED
//If you are using Commodore's chargen ROM this will double the amount of lines of text on the OLED
i2cLcdUseCBMChar = 1

//When using this option Pi1541 will lower case all file names sent back to the computer
//This can be useful when using FB as it will in-turn display all file names in upper case.
lowercaseBrowseModeFilenames = 1

//ROTARY:
//
// KY-040 Rotary Encoder Support
//
//    If you would like to use a KY-040 Rotary Encoder for browse menu up/down
//    and select, you can enable it here.  Connect as follows:
//
//       GPIO 22  -  Menu up       -  Encoder pin A (CLK)
//       GPIO 23  -  Menu down     -  Encoder pin B (DT)
//       GPIO 27  -  Enter/Select  -  Encoder pushbutton (SW)
//
//    ** Using an encoder is incompatible with the button remapping.  You must
//       use the default values of Enter=1, Up=2, Down=3, Back=4 and Insert=5.
//
//    ** This has only been tested using a Raspberry Pi 3.  Earlier models may
//       or may not work as expected!
//
//    Please see dmRotary.h for full implementation details.
//
//RotaryEncoderEnable = 1

// This option will display the temperature of the Pi's CPU.
// It should be about 52°C anything above 65°C is bad and there is something wrong with your hardware
DisplayTemperature = 1

// This option will display a visualisation of the data of a disk image on the Pi's HDMI screen.
DisplayTracks = 1
